# Static Timing Analysis

Project : | VEML6031X00
Build Time : | 06/06/23 15:24:49
Device : | CY8C5888LTI-LP097
Temperature : | -40C - 85/125C
VDDA : | 5.00
VDDABUF : | 5.00
VDDD : | 5.00
VDDIO0 : | 5.00
VDDIO1 : | 5.00
VDDIO2 : | 5.00
VDDIO3 : | 5.00
VUSB : | 5.00
Voltage : | 5.0

Expand All | Collapse All | Show All Paths | Hide All Paths
+ Timing Violation Section
No Timing Violations
+ Clock Summary Section

Clock | Domain | Nominal Frequency | Required Frequency | Maximum Frequency | Violation
--- | --- | --- | --- | --- | ---
ClockBlock/clk_bus_glb_ff | ClockBlock/clk_bus_glb_ff | UNKNOWN | UNKNOWN | N/A |
CyILO | CyILO | 100.000 kHz | 100.000 kHz | N/A |
CyIMO | CyIMO | 24.000 MHz | 24.000 MHz | N/A |
CyMASTER_CLK | CyMASTER_CLK | 24.000 MHz | 24.000 MHz | N/A |
CyBUS_CLK | CyMASTER_CLK | 24.000 MHz | 24.000 MHz | N/A |
CyPLL_OUT | CyPLL_OUT | 24.000 MHz | 24.000 MHz | N/A |

+ Clock To Output Section
+ ClockBlock/clk_bus_glb_ff

Source | Destination | Delay (ns)
--- | --- | ---
\I2C_1:I2C_FF\/sda_out | SDA_1(0)_PAD:out | 24.751
Type | Location | Fanout | Instance/Net | Source | Dest | Delay (ns)
--- | --- | --- | --- | --- | --- | ---
i2ccell | F(I2C,0) | 1 | \I2C_1:I2C_FF\ | \I2C_1:I2C_FF\/clock | \I2C_1:I2C_FF\/sda_out | 1.000
Route |  | 1 | \I2C_1:sda_x_wire\ | \I2C_1:I2C_FF\/sda_out | SDA_1(0)/pin_input | 7.818
iocell2 | P12[1] | 1 | SDA_1(0) | SDA_1(0)/pin_input | SDA_1(0)/pad_out | 15.933
Route |  | 1 | SDA_1(0)_PAD | SDA_1(0)/pad_out | SDA_1(0)_PAD:out | 0.000
Clock |  |  |  |  | Clock path delay | 0.000
\I2C_1:I2C_FF\/scl_out | SCL_1(0)_PAD:out | 24.669
Type | Location | Fanout | Instance/Net | Source | Dest | Delay (ns)
--- | --- | --- | --- | --- | --- | ---
i2ccell | F(I2C,0) | 1 | \I2C_1:I2C_FF\ | \I2C_1:I2C_FF\/clock | \I2C_1:I2C_FF\/scl_out | 1.000
Route |  | 1 | \I2C_1:Net_643_0\ | \I2C_1:I2C_FF\/scl_out | SCL_1(0)/pin_input | 7.814
iocell1 | P12[0] | 1 | SCL_1(0) | SCL_1(0)/pin_input | SCL_1(0)/pad_out | 15.855
Route |  | 1 | SCL_1(0)_PAD | SCL_1(0)/pad_out | SCL_1(0)_PAD:out | 0.000
Clock |  |  |  |  | Clock path delay | 0.000